This is the source configuration of the MBE. The port numbers here correspond to the
values in the shutter status data (e.g. GMx_Shutter_Control.Value.txt). Each shutter
port has a binary value that is added up to give the logged data value. Port 1 
corresponds to a value of 1, port 2 => 2, port 3 => 4, port 4 => 16 etc.

O3_Nozzle_IonGauge on port 10
O3_Nozzle_Baratron on port 10
O3_Nozzle_RGA on port 10
O3_Nozzle_Direct on port 10
Side_Inlet_IonGauge on port 10
Side_Inlet_Baratron on port 10
Side_Inlet_RGA on port 10
Side_Inlet_Direct on port 10
Bi_base on port 2
Bi_tip on port 2
Sr_base on port 5
Sr_tip on port 5
Nb2O5base on port 6
Au_base on port 8
Au_tip on port 8
Ta2O5base on port 7
GM1_TELEMARK_EBEAM_base on port 11
EIES_Channel1_Rate on port 11
N2_Plasma_RF_Forward on port 1
N2_Plasma_RF_TuningCap on port 1
N2_Plasma_RF_LoadCap on port 1
K_Base on port 4
K_Tip on port 4
