This is the source configuration of the MBE. The port numbers here correspond to the
values in the shutter status data (e.g. GMx_Shutter_Control.Value.txt). Each shutter
port has a binary value that is added up to give the logged data value. Port 1 
corresponds to a value of 1, port 2 => 2, port 3 => 4, port 4 => 16 etc.

O3_Nozzle_IonGauge on port 2
O3_Nozzle_Baratron on port 2
O3_Nozzle_RGA on port 2
O3_Nozzle_Direct on port 2
InOx_tip on port 7
InOx_base on port 7
EBeam_zone on port 11
Newzone on port 11
SiO_base on port 6
GaOx_tip on port 3
GaOx_base on port 3
Ba_tip on port 8
Ba_base on port 8
Y_base on port 9
SnO2_tip on port 4
SnO2_base on port 4
La_base on port 5
Sr_tip on port 10
Sr_base on port 10
