<?xml version="1.0"?>
<xrdMeasurements xmlns="http://www.xrdml.com/XRDMeasurement/2.2" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:schemaLocation="http://www.xrdml.com/XRDMeasurement/2.2 http://www.xrdml.com/XRDMeasurement/2.2/XRDMeasurement.xsd" status="Completed" recordIdentifier="{6BF7BCA3-B723-48D5-8A75-19B04BF17F84}">
	<comment>
		<entry>Configuration=Chi-Phi-z Stage 240 mm (reflection), Owner=schlomgroup, Creation date=10/25/2021 3:07:32 PM</entry>
		<entry>Goniometer=Theta/Theta; Minimum step size 2Theta:0.0001; Minimum step size Omega:0.0001</entry>
		<entry>Sample stage=Chi-Phi-z stage 240 mm (reflection); Minimum step size Phi:0.01; Minimum step size Chi:0.01; Minimum step size Z:0.001</entry>
		<entry>Diffractometer system=EMPYREAN</entry>
		<entry>Measurement program=C:\PANalytical\Data Collector\Programs\Chris_Parzyck\XRR\XRR_4_min_1ch.xrdmp, Created identifier={A57FA78C-849E-48F1-A7A0-A6B0D3CE0C82}, Created by=schlomgroup, Id=WL:DESKTOP-FMVO1QA:schlomgroup, Creation date=6/30/2022 9:46:26 PM, Modified identifier={2DCED973-DDE8-41F5-A45D-1E5543DE6BDC}, Modified by=schlomgroup, Id=WL:DESKTOP-FMVO1QA:schlomgroup, Modification date=7/8/2022 4:47:24 PM</entry>
		<entry>Batch program=C:\PANalytical\Data Collector\Programs\Chris_Parzyck\Scripts\STO_align_wtth_42_54_5ch_6min+XRR.xrdmp, Created identifier={7020229A-94F3-469E-87B3-2E48492D722C}, Created by=schlomgroup, Id=WL:DESKTOP-FMVO1QA:schlomgroup, Creation date=3/24/2022 8:53:15 PM, Modified identifier={F4561AD7-D86C-431E-B67C-CBB7CB13BFF7}, Modified by=schlomgroup, Id=WL:DESKTOP-FMVO1QA:schlomgroup, Modification date=7/8/2022 4:51:21 PM</entry>
	</comment>
	<sample type="To be analyzed">
		<id>CY230116C</id>
		<name>Christopher Parzyck</name>
		<preparedBy></preparedBy>
	</sample>
	<xrdMeasurement measurementType="Scan" status="Completed" sampleMode="Reflection">
		<comment>
			<entry>PHD Lower Level = 4.02 (keV), PHD Upper Level = 16.10 (keV)</entry>
		</comment>
		<usedWavelength intended="K-Alpha 1">
			<kAlpha1 unit="Angstrom">1.5405980</kAlpha1>
			<kAlpha2 unit="Angstrom">1.5444260</kAlpha2>
			<kBeta unit="Angstrom">1.3922500</kBeta>
			<ratioKAlpha2KAlpha1>0.0000</ratioKAlpha2KAlpha1>
		</usedWavelength>
		<incidentBeamPath>
			<radius unit="mm">240.00</radius>
			<xRayTube id="1010048" name="Empyrean Cu LFF HR (9430 033 7310x) DK433060">
				<tension unit="kV">45.0</tension>
				<current unit="mA">40.0</current>
				<anodeMaterial>Cu</anodeMaterial>
				<focus type="Line">
					<length unit="mm">12.0</length>
					<width unit="mm">0.4</width>
					<takeOffAngle unit="deg">4.4</takeOffAngle>
				</focus>
			</xRayTube>
			<xRayMirror id="27080001" name="Inc. Beam Cu W/Si (hybrid MPD)" hybrid="true">
				<crystal type="Graded" shape="Parabolic">W/Si</crystal>
				<acceptanceAngle unit="deg">0.800</acceptanceAngle>
				<length unit="mm">55.3</length>
			</xRayMirror>
			<monochromator id="23090002" name="Hybrid monochr. 2xGe220 Cu asym." hybrid="true">
				<crystal type="Asymmetric" shape="Flat">Ge</crystal>
				<numberOfReflections>2</numberOfReflections>
				<hkl>
					<h>2</h>
					<k>2</k>
					<l>0</l>
				</hkl>
			</monochromator>
			<divergenceSlit id="22010004" name="Fixed slit 1/2°" xsi:type="fixedDivergenceSlitType">
				<distanceToSample unit="mm">179.30</distanceToSample>
				<height unit="mm">0.76</height>
			</divergenceSlit>
		</incidentBeamPath>
		<sampleOffset>
			<position axis="2Theta" unit="deg">0.0678</position>
			<position axis="Omega" unit="deg">-0.0409</position>
			<position axis="Chi" unit="deg">0.22</position>
		</sampleOffset>
		<diffractedBeamPath>
			<radius unit="mm">240.00</radius>
			<detector id="7010020" name="PIXcel3D-Medipix3 1x1 detector" xsi:type="areaDetectorType">
				<phd unit="%">
					<lowerLevel>25.0</lowerLevel>
					<upperLevel>100.0</upperLevel>
				</phd>
				<mode>Receiving slit</mode>
				<activeChannelsEquatorial>1</activeChannelsEquatorial>
				<activeChannelsAxial>255</activeChannelsAxial>
				<pitchEquatorial unit="mm">0.05500</pitchEquatorial>
				<pitchAxial unit="mm">0.05500</pitchAxial>
				<readOutPeriod unit="seconds">0.050</readOutPeriod>
			</detector>
		</diffractedBeamPath>
		<scan appendNumber="0" mode="Continuous" scanAxis="Omega-2Theta" status="Completed">
			<header>
				<startTimeStamp>2023-01-16T21:46:01-05:00</startTimeStamp>
				<endTimeStamp>2023-01-16T21:50:15-05:00</endTimeStamp>
				<author>
					<name>schlomgroup</name>
				</author>
				<source>
					<applicationSoftware version="7.2a">Data Collector</applicationSoftware>
					<instrumentControlSoftware version="8.2  20201204">EMPYREAN</instrumentControlSoftware>
					<instrumentID>0000000011261638</instrumentID>
				</source>
			</header>
			<dataPoints>
				<positions axis="2Theta" unit="deg">
					<startPosition>-0.1356</startPosition>
					<endPosition>9.8844</endPosition>
				</positions>
				<positions axis="Omega" unit="deg">
					<startPosition>-0.0150</startPosition>
					<endPosition>4.9950</endPosition>
				</positions>
				<positions axis="Phi" unit="deg">
					<commonPosition>0.00</commonPosition>
				</positions>
				<positions axis="Chi" unit="deg">
					<commonPosition>0.00</commonPosition>
				</positions>
				<positions axis="Z" unit="mm">
					<commonPosition>9.434</commonPosition>
				</positions>
				<commonCountingTime unit="seconds">0.440</commonCountingTime>
				<counts unit="counts">1030 1059 1037 1217 2061 3627 228694 4295932 8272846 9090120 8723572 8437420 8538332 8001399 5596600 2272116 700967 515753 548372 588711 628582 667836 707039 743264 780198 812409 846276 875874 905369 930005 956337 973755 992868 1005883 1013450 1012215 998250 952042 852724 716435 614981 542110 486735 438658 397860 361282 329320 298579 273583 247936 223433 203117 181851 165531 146944 132654 119874 106225 95133 84704 74816 65890 58404 50993 44779 39198 34592 29815 25862 22446 19677 17025 14968 13084 11643 10356 9030 8328 7653 6958 6566 6347 6101 6025 5866 5886 5791 5826 5902 6045 6096 6091 6129 6249 6156 6141 6267 6262 6233 6082 5984 5945 5871 5767 5742 5857 5729 5566 5251 5024 4645 4197 3868 3560 3162 3091 2844 2710 2383 2272 2101 1856 1713 1551 1455 1270 1211 1126 1001 869 812 772 727 700 568 603 518 526 497 490 518 523 551 538 568 555 554 590 610 631 642 606 625 619 659 689 693 650 587 712 613 600 628 581 629 547 564 566 511 502 460 468 396 414 376 348 312 297 282 243 248 203 202 161 170 132 141 119 128 90 100 83 91 88 82 69 77 76 80 63 85 63 85 80 73 97 94 102 89 89 118 94 114 119 97 97 109 113 128 103 131 117 106 109 95 101 82 86 78 81 77 86 81 69 76 59 65 64 54 65 45 43 44 49 57 35 33 33 29 32 28 26 25 26 33 32 27 30 24 25 24 27 32 24 25 34 34 26 27 32 36 37 23 41 33 40 21 33 32 29 44 44 30 31 36 30 29 24 34 34 28 30 23 30 21 29 13 23 27 26 16 22 23 18 15 28 18 13 22 11 16 10 27 18 14 18 16 15 18 17 14 30 15 21 15 10 15 19 23 12 20 20 19 14 30 19 15 19 21 23 19 13 21 15 15 17 17 17 14 13 16 10 24 16 18 10 16 13 20 14 16 14 14 18 14 15 15 11 5 16 15 11 13 17 12 12 16 13 9 11 15 12 12 8 6 14 12 11 11 16 17 7 10 13 6 13 17 13 11 11 7 17 9 8 15 10 11 13 10 9 14 8 11 13 7 14 14 10 10 10 9 14 12 8 8 8 3 17 11 10 6 9 8 12 15 11 11 11 11 13 15 8 4 10 13 8 15 7 6 10 11 6 10 9 9 11 9 9 8 12 15 8 12 9 11 12 10 8 8 10 8 8 9 8 8 5 14 9 9 8 3 11 7 8 7 9 7 13 7 6 5 10 5 2 5 11 6 6 10 6 9 5</counts>
			</dataPoints>
		</scan>
	</xrdMeasurement>
</xrdMeasurements>
